
MANUAL VALVE UNDER MONITOR
Task Force Tips VUM, model # AKP13B11CZ manually controlled monitor valve shall be provided under the monitor. The valve shall be controlled with an NFPA compliant slow-close crank handle gear operator. A position indicator shall be provided to allow for quick visualization of the status of the valve in the open, closed or partial positions. The unit shall have a flow capability of up to 2000 GPM with friction loss no more than 6 psi. For maximum corrosion protection the aluminum casting shall be hardcoat anodized, with a silver powder coat internal and external finish. The valve ball shall be stainless steel. The unit shall have a unique serial number and be covered by a five-year warranty.
The valve shall be configured with a 4” ANSI 150 flange inlet and 4” ANSI 150 flange outlet. Ports C1 shall have a left hand elbow quarter turn valve with2-1/2” NH male outlet installed, extended 4-3/4” from main valve. Ports C2 and C3 shall have blind plugs installed. Port C4 shall have a right hand elbow quarter turn valve with 2-1/2” NH male outlet installed, extended 4-3/4” from main valve. All 2-1/2” NH male discharges shall have a 2-1/2” NH female by 1-1/2” NH male thread reducer and a 1-1/2” NH female cap with lanyard.

